{"text_format":"1","workbook":"xlsx","n_sheets":8,"sheets":["About","CMV20000","CMV12000 ","IMX174","IMX250","IMX252","IMX253","IMX255"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"About","index":0,"n_rows":9,"n_cols":1,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["XIMEA Camera sensor performance caluclator"]
["Version 2016-05-23"]
[]
["This document contains multiple calculators for different sensors. Each is located in different sheet."]
[]
["Usage:"]
["1. Activate the sheet depending on sensor."]
["2. Fill settings (orange)"]
["3. Use results (green)"]

{"sheet":"CMV20000","index":1,"n_rows":18,"n_cols":8,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["Setting","Value","Units","min","max","Note"]
["Sensor Readout Frequency",480,"[MHz]",120,480,"Data Rate of Sensor image data output"]
["Bit Depth",12,"[count]",12,12,"CMV20000 supports only 12 output; In this example Transport Packing == Sensor Bit Depth == 12bit"]
["ROI Width",5120,"[count]",16,5120,"ROI in X direction decreases average transport bandwidth needed to transfer one frame (the whole line is read from sensor but only ROI part is sent)"]
["ROI Height",3840,"[count]",2,3840,"ROI in Y direction decreases frame readout time (decreases number of lines that need to be read out before going to next frame)"]
["Exp time",1500,"[count]",1,65535,"Actual Exposure Time depends on the Exp_Time, FOT and Clk_freq"]
[]
["Results"]
["Frame Transfer",null,null,null,null,"Calculations"]
["Pixel Count",{"$f":"B5*B4/1000000","v":19.660799999999998},"[Mpix]",null,null,"master clock",{"$f":"B2/12","v":40},"[MHz]"]
["Image Size",{"$f":"B4*B5/8*B3/1000000","v":29.491199999999999},"[MBytes]",null,null,"master clk_per",{"$f":"1000/G10","v":25},"[ns]"]
["Frame Time",{"$f":"MAX(G13,B18)+G13/1000","v":30.798767999999999},"[ms]",null,null,"FOT",{"$f":"((80*80+80/8)+2*641)*G11/1000","v":192.3},"[us]"]
["Max FPS",{"$f":"1000/B12","v":32.468831220781297},"[count]",null,null,"Readout Time",{"$f":"641*G11*B5/2/1000000","v":30.768000000000001},"[ms]"]
["Average Transfer Speed",{"$f":"B11/B12*1000","v":957.54479529830553},"[MB/s]"]
[]
["Exposure times"]
["Min Exposure Time",{"$f":"(1+47*80)*G11/1000","v":94.025000000000006},"[us]"]
["Actual Exposure Time",{"$f":"((B6-1)*641+1+47*80)*G11/1000000","v":24.115500000000001},"[ms]"]

{"sheet":"CMV12000 ","index":2,"n_rows":30,"n_cols":18,"rows_kept":30,"cut":false,"hidden":false,"merged":[]}
["Setting","Value","Units","min","max","Note"]
["Camera Model","CB120",null,null,null,"CB120xG-CM has PCIe x4 Gen2 interface (1750MB/s); CB120xG-CM-X8G3 with PCIe x8 Gen3 interface (7000MB/s)"]
["Sensor Readout Frequency",400,"[MHz]",120,600,"Data Rate of Sensor image data output; Note: CB120 camera implementation has 480MHz limit @8bit mode"]
["Bit Depth",10,"[count]",8,12,"In this example Camera Transport Packing == Sensor Bit Depth"]
["Acquisition Mode","Normal","[count]"]
["Channel Count per Side",16,"[count]",null,null,"CB120 supports only 16 Channels per side; CB120-X8G3 support only 32 Channels per side"]
["ROI Width",4096,"[count]",16,4096,"ROI in X direction decreases average transport bandwidth needed to transfer one frame (the whole line is read from sensor but only ROI part is sent)"]
["ROI Height",3072,"[count]",2,3072,"ROI in Y direction decreases frame readout time (decreases number of lines that need to be read out before going to next frame)"]
["Exp time reg",1548,"[count]",1,65535,"See the resulting Actual Exposure Time in [ms] below (depends on the Exp_Time, FOT and Clk_freq)"]
["Exp time ",10.001125,"[ms]",{"$f":"((1-1)*(G18+1)+(34*MOD(G17,256))+1)*G13*B4/1000000","v":2.2974999999999999E-2},{"$f":"((65535-1)*(G18+1)+(34*MOD(G17,256))+1)*G13*B4/1000000","v":422.71727499999997}]
["Results",null,null,null,null,null,null,null,null,null,"Register Presets"]
["Frame Transfer",null,null,null,null,"Calculations",null,null,null,null,"Channel Count",null,32,16,8,4,2,1]
["Pixel Count",{"$f":"B8*B7/1000000","v":12.582912},"[Mpix]",null,null,"clk_per",{"$f":"1000/B3","v":2.5},"[ns]",null,"8bit","Normal","reg82",3618,2082,1058,546,290,290]
["Image Size",{"$f":"B7*B8/8*B4/1000000","v":15.72864},"[MBytes]",null,null,"channel count log",{"$f":"LOG(B6,2)","v":4},"[count]",null,null,null,"reg85",143,257,515,1031,2063,4127]
["Frame Time",{"$f":"MAX(G22,B21)+G19/1000","v":10.052725000000001},"[ms]",null,null,"mode number",{"$f":"ISNUMBER(FIND(B5,\"Normal\"))*1+ISNUMBER(FIND(B5,\"Skipping 2x2\"))*2+ISNUMBER(FIND(B5,\"Binning 2x2\"))*3","v":1},"[count]",null,null,"Subsample 2x2","reg82",2338,2082,1058,546,290,290]
["Max FPS",{"$f":"1000/B15","v":99.475515345341677},"[count]",null,null,"bit depth number",{"$f":"(B4-8)/2","v":1},"[count]",null,null,null,"reg85",239,257,515,1031,2063,4127]
["Average Transfer Speed",{"$f":"B14/B15*1000","v":1564.6145696813549},"[MB/s]",null,null,"reg 82",{"$f":"INDIRECT(ADDRESS(13+2*(G15-1)+6*G16,13+5-G14))","v":1563},"[count]",null,null,"Binning 2x2","reg82",802,802,802,546,290,290]
[null,null,null,null,null,"reg 85",{"$f":"INDIRECT(ADDRESS(14+2*(G15-1)+6*G16,13+5-G14))","v":257},"[count]",null,null,null,"reg85",767,767,767,1031,2063,4127]
[null,null,null,null,null,"FOT",{"$f":"(INT(G17/256)+2)*G20","v":51.6},"[us]",null,"10bit","Normal","reg82",3099,1563,795,539,283,283]
["Exposure times",null,null,null,null,"Line Time",{"$f":"(G18+1)*G13*B4/1000","v":6.45},"[us]",null,null,null,"reg85",128,257,515,1031,2063,4127]
["Actual Exposure Time",{"$f":"((B9-1)*(G18+1)+(34*MOD(G17,256))+1)*G13*B4/1000000","v":10.001125},"[ms]",null,null,"Readout lines",3072,"[count]",null,null,"Subsample 2x2","reg82",2843,1563,795,539,283,283]
[null,null,null,null,null,"Readout time",{"$f":"G20*G21/2/1000","v":9.9072000000000013},"[ms]",null,null,null,"reg85",143,257,515,1031,2063,4127]
[null,null,null,null,null,null,null,null,null,null,"Binning 2x2","reg82",798,798,798,542,286,286]
[null,null,null,null,null,null,null,null,null,null,null,"reg85",575,575,575,1031,2063,4127]
[null,null,null,null,null,null,null,null,null,"12bit","Normal","reg82",1822,1822,1054,542,286,286]
[null,null,null,null,null,null,null,null,null,null,null,"reg85",244,257,515,1031,2063,4127]
[null,null,null,null,null,null,null,null,null,null,"Subsample 2x2","reg82",2078,3102,1054,542,286,286]
[null,null,null,null,null,null,null,null,null,null,null,"reg85",239,257,515,1031,2063,4127]
[null,null,null,null,null,null,null,null,null,null,"Binning 2x2","reg82",1054,1054,1054,542,286,286]
[null,null,null,null,null,null,null,null,null,null,null,"reg85",479,479,515,1031,2063,4127]

{"sheet":"IMX174","index":3,"n_rows":18,"n_cols":15,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["Setting","Value","Units","min","max","Note"]
["Bit Depth",10,"[count]",10,12,"IMX174 supports 10 and 12 bit depth"]
["Channel count",8,"[count]",null,null,"IMX174 supports 2; 4; or 8 channels"]
["ROI Width",1936,"[count]",8,1936,"ROI in X direction decreases average transport bandwidth needed to transfer one frame (the whole line is read from sensor but only ROI part is sent)"]
["ROI Height",1216,"[count]",2,1216,"ROI in Y direction decreases frame readout time (decreases number of lines that need to be read out before going to next frame)"]
["Exp time",19,"[us]",{"$f":"B17","v":19},{"$f":"ROUND(65535*(1/75000000)*1000000*4085+13.73, 0)","v":3569487}]
[]
["Results"]
["Frame Transfer",null,null,null,null,"Calculations",null,null,null,null,"Register Presets"]
["Pixel Count",{"$f":"B5*B4/1000000","v":2.3541759999999998},"[Mpix]",null,null,"bit depth number",{"$f":"(B2-8)/2","v":1},"[count]",null,null,"Channel Count",null,8,4,2]
["Image Size",{"$f":"B4*B5/8*B2/1000000","v":2.94272},"[MBytes]",null,null,"channel count log",{"$f":"LOG(B3,2)","v":3},"[count]",null,"10bit","Normal","HMAX",360,720,1440]
["Frame Time",{"$f":"G14*G13/1000","v":6.0192000000000005},"[ms]",null,null,"HMAX reg",{"$f":"MAX(INDIRECT(ADDRESS(G10*2+9,16-G11)),ROUND((B6-13.73)/4085/((1/75000000)*1000000), 0))","v":360},"[count]"]
["Max FPS",{"$f":"1000/B12","v":166.13503455608716},"[count]",null,null,"H period",{"$f":"(1/75000000)*1000000*G12","v":4.8000000000000007},"[us]",null,"12bit","Normal","HMAX",462,924,1848]
["Average Transfer Speed",{"$f":"B11/B12*1000","v":488.8888888888888},"[MB/s]",null,null,"VMAX reg",{"$f":"MAX(ROUND((((B6-13.73)/G13)+10), 0), B5+38)","v":1254},"[count]"]
[null,null,null,null,null,"FOT",{"$f":"10*G13","v":48.000000000000007},"[us]"]
["Exposure times",null,null,null,null,"Readout Time",{"$f":"G13*B5/1000","v":5.8368000000000011},"[ms]"]
["Min Exposure Time",{"$f":"ROUND(INDIRECT(ADDRESS(G10*2+9,16-G11))*(1/75000000)*1000000+13.73, 0)","v":19},"[us]"]
["Actual Exposure Time",{"$f":"((ROUND((B6-13.73)/G13,0)*G13)+13.73)/1000","v":1.8530000000000001E-2},"[ms]"]

{"sheet":"IMX250","index":4,"n_rows":21,"n_cols":15,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["Setting","Value","Units","min","max","Note"]
["Sensor type","Mono",null,null,null,"Only Mono IMX250 supports Binning"]
["Bit Depth",8,"[count]",8,12,"IMX250 supports 8; 10 and 12 bit depth"]
["Binning","1x1",null,null,null,"Binning/Decimation: vertical x horizontal"]
["Decimation","1x1"]
["Channel count",16,"[count]",null,null,"IMX250 supports 4; 8; or 16 channels"]
["ROI Width",2464,"[count]",8,2464,"ROI in X direction decreases average transport bandwidth needed to transfer one frame (the whole line is read from sensor but only ROI part is sent)"]
["ROI Height",2056,"[count]",4,2056,"ROI in Y direction decreases frame readout time (decreases number of lines that need to be read out before going to next frame)"]
["Exp time",19,"[us]",{"$f":"B20","v":17},{"$f":"ROUND(65535*(1/75000000)*1000000*4085+13.73, 0)","v":3569487}]
[]
["Results"]
["Frame Transfer",null,null,null,null,"Calculations",null,null,null,null,"Register Presets"]
["Pixel Count",{"$f":"B8*B7/1000000","v":5.0659840000000003},"[Mpix]",null,null,"bit depth number",{"$f":"(B3-6)/2","v":1},"[count]",null,null,"Channel Count",null,16,8,4]
["Image Size",{"$f":"B7*B8/8*B3/1000000","v":5.0659840000000003},"[MBytes]",null,null,"channel count log",{"$f":"LOG(B6,2)","v":4},"[count]",null,"8bit","Normal","HMAX",217,360,676]
["Frame Time",{"$f":"G17*G16/1000","v":6.0586400000000005},"[ms]",null,null,"HMAX reg",{"$f":"INDIRECT(ADDRESS((G13*2+12)+ISNUMBER(FIND(\"x2\",B5, 2))*1, 17-G14))","v":217},"[count]",null,null,"Decimation Xx2","HMAX",218,218,368]
["Max FPS",{"$f":"1000/B15","v":165.05354336946905},"[count]",null,null,"H period",{"$f":"(1/75000000)*1000000*G15","v":2.8933333333333335},"[us]",null,"10bit","Normal","HMAX",245,440,835]
["Average Transfer Speed",{"$f":"B14/B15*1000","v":836.1586098530363},"[MB/s]",null,null,"VMAX reg",{"$f":"MAX(ROUND((((B9-13.73)/G16)+10), 0), B8+38)","v":2094},"[count]",null,null,"Decimation Xx2","HMAX",260,250,450]
[null,null,null,null,null,"FOT",{"$f":"10*G16","v":28.933333333333337},"[us]",null,"12bit","Normal","HMAX",396,519,996]
["Exposure times",null,null,null,null,"Readout Time",{"$f":"G16*B8/1000","v":5.9486933333333338},"[ms]",null,null,"Decimation Xx2","HMAX",396,396,534]
["Min Exposure Time",{"$f":"ROUND(G15*(1/75000000)*1000000+13.73, 0)","v":17},"[us]"]
["Actual Exposure Time",{"$f":"((ROUND((B9-13.73)/G16,0)*G16)+13.73)/1000","v":1.9516666666666665E-2},"[ms]"]

{"sheet":"IMX252","index":5,"n_rows":21,"n_cols":15,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["Setting","Value","Units","min","max","Note"]
["Sensor type","Mono",null,null,null,"Only Mono IMX252 supports Binning"]
["Bit Depth",8,"[count]",8,12,"IMX252 supports 8; 10 and 12 bit depth"]
["Binning","1x1",null,null,null,"Binning/Decimation: vertical x horizontal"]
["Decimation","1x1"]
["Channel count",16,"[count]",null,null,"IMX252 supports 4; 8; or 16 channels"]
["ROI Width",2064,"[count]",8,2064,"ROI in X direction decreases average transport bandwidth needed to transfer one frame (the whole line is read from sensor but only ROI part is sent)"]
["ROI Height",1544,"[count]",4,1544,"ROI in Y direction decreases frame readout time (decreases number of lines that need to be read out before going to next frame)"]
["Exp time",19,"[us]",{"$f":"B20","v":17},{"$f":"ROUND(65535*(1/75000000)*1000000*4085+13.73, 0)","v":3569487}]
[]
["Results"]
["Frame Transfer",null,null,null,null,"Calculations",null,null,null,null,"Register Presets"]
["Pixel Count",{"$f":"B8*B7/1000000","v":3.1868159999999999},"[Mpix]",null,null,"bit depth number",{"$f":"(B3-6)/2","v":1},"[count]",null,null,"Channel Count",null,16,8,4]
["Image Size",{"$f":"B7*B8/8*B3/1000000","v":3.1868159999999999},"[MBytes]",null,null,"channel count log",{"$f":"LOG(B6,2)","v":4},"[count]",null,"8bit","Normal","HMAX",217,310,576]
["Frame Time",{"$f":"G17*G16/1000","v":4.5772533333333341},"[ms]",null,null,"HMAX reg",{"$f":"INDIRECT(ADDRESS((G13*2+12)+ISNUMBER(FIND(\"x2\",B5, 2))*1, 17-G14))","v":217},"[count]",null,null,"Decimation Xx2","HMAX",217,218,320]
["Max FPS",{"$f":"1000/B15","v":218.47163073051084},"[count]",null,null,"H period",{"$f":"(1/75000000)*1000000*G15","v":2.8933333333333335},"[us]",null,"10bit","Normal","HMAX",245,380,710]
["Average Transfer Speed",{"$f":"B14/B15*1000","v":696.22888835808362},"[MB/s]",null,null,"VMAX reg",{"$f":"MAX(ROUND((((B9-13.73)/G16)+10), 0), B8+38)","v":1582},"[count]",null,null,"Decimation Xx2","HMAX",245,245,390]
[null,null,null,null,null,"FOT",{"$f":"10*G16","v":28.933333333333337},"[us]",null,"12bit","Normal","HMAX",396,444,846]
["Exposure times",null,null,null,null,"Readout Time",{"$f":"G16*B8/1000","v":4.4673066666666674},"[ms]",null,null,"Decimation Xx2","HMAX",396,396,456]
["Min Exposure Time",{"$f":"ROUND(G15*(1/75000000)*1000000+13.73, 0)","v":17},"[us]"]
["Actual Exposure Time",{"$f":"((ROUND((B9-13.73)/G16,0)*G16)+13.73)/1000","v":1.9516666666666665E-2},"[ms]"]

{"sheet":"IMX253","index":6,"n_rows":21,"n_cols":15,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["Setting","Value","Units","min","max","Note"]
["Sensor type","Mono",null,null,null,"Only Mono IMX253 supports Binning"]
["Bit Depth",8,"[count]",8,12,"IMX253 supports 8; 10 and 12 bit depth"]
["Binning","1x1",null,null,null,"Binning/Decimation: vertical x horizontal"]
["Decimation","1x1"]
["Channel count",16,"[count]",null,null,"IMX253 supports 4; 8; or 16 channels"]
["ROI Width",4112,"[count]",8,4112,"ROI in X direction decreases average transport bandwidth needed to transfer one frame (the whole line is read from sensor but only ROI part is sent)"]
["ROI Height",3008,"[count]",4,3008,"ROI in Y direction decreases frame readout time (decreases number of lines that need to be read out before going to next frame)"]
["Exp time",19,"[us]",{"$f":"B20","v":19},{"$f":"ROUND(65535*(1/75000000)*1000000*4085+14.26, 0)","v":3569487}]
[]
["Results"]
["Frame Transfer",null,null,null,null,"Calculations",null,null,null,null,"Register Presets"]
["Pixel Count",{"$f":"B8*B7/1000000","v":12.368895999999999},"[Mpix]",null,null,"bit depth number",{"$f":"(B3-6)/2","v":1},"[count]",null,null,"Channel Count",null,16,8,4]
["Image Size",{"$f":"B7*B8/8*B3/1000000","v":12.368895999999999},"[MBytes]",null,null,"channel count log",{"$f":"LOG(B6,2)","v":4},"[count]",null,"8bit","Normal","HMAX",355,568,1092]
["Frame Time",{"$f":"G17*G16/1000","v":14.417733333333334},"[ms]",null,null,"HMAX reg",{"$f":"INDIRECT(ADDRESS((G13*2+12)+ISNUMBER(FIND(\"x2\",B5, 2))+ISNUMBER(FIND(\"x2\",B4, 2)), 17-G14))","v":355},"[count]",null,null,"Decimation Xx2","HMAX",355,356,576]
["Max FPS",{"$f":"1000/B15","v":69.359030083323304},"[count]",null,null,"H period",{"$f":"(1/75000000)*1000000*G15","v":4.7333333333333334},"[us]",null,"10bit","Normal","HMAX",375,700,1355]
["Average Transfer Speed",{"$f":"B14/B15*1000","v":857.8946297614973},"[MB/s]",null,null,"VMAX reg",{"$f":"MAX(ROUND((((B9-13.73)/G16)+10), 0), B8+38)","v":3046},"[count]",null,null,"Decimation Xx2","HMAX",375,380,710]
[null,null,null,null,null,"FOT",{"$f":"10*G16","v":47.333333333333336},"[us]",null,"12bit","Normal","HMAX",522,831,1614]
["Exposure times",null,null,null,null,"Readout Time",{"$f":"G16*B8/1000","v":14.237866666666667},"[ms]",null,null,"Decimation Xx2","HMAX",522,522,846]
["Min Exposure Time",{"$f":"ROUND(G15*(1/75000000)*1000000+14.26, 0)","v":19},"[us]"]
["Actual Exposure Time",{"$f":"((ROUND((B9-14.26)/G16,0)*G16)+14.26)/1000","v":1.8993333333333331E-2},"[ms]"]

{"sheet":"IMX255","index":7,"n_rows":21,"n_cols":15,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["Setting","Value","Units","min","max","Note"]
["Sensor type","Mono",null,null,null,"Only Mono IMX255 supports Binning"]
["Bit Depth",8,"[count]",8,12,"IMX255 supports 8; 10 and 12 bit depth"]
["Binning","1x1",null,null,null,"Binning/Decimation: vertical x horizontal"]
["Decimation","1x1"]
["Channel count",16,"[count]",null,null,"IMX255 supports 4; 8; or 16 channels"]
["ROI Width",4112,"[count]",8,4112,"ROI in X direction decreases average transport bandwidth needed to transfer one frame (the whole line is read from sensor but only ROI part is sent)"]
["ROI Height",2176,"[count]",4,2176,"ROI in Y direction decreases frame readout time (decreases number of lines that need to be read out before going to next frame)"]
["Exp time",19,"[us]",{"$f":"B20","v":19},{"$f":"ROUND(65535*(1/75000000)*1000000*4085+14.26, 0)","v":3569487}]
[]
["Results"]
["Frame Transfer",null,null,null,null,"Calculations",null,null,null,null,"Register Presets"]
["Pixel Count",{"$f":"B8*B7/1000000","v":8.9477119999999992},"[Mpix]",null,null,"bit depth number",{"$f":"(B3-6)/2","v":1},"[count]",null,null,"Channel Count",null,16,8,4]
["Image Size",{"$f":"B7*B8/8*B3/1000000","v":8.9477119999999992},"[MBytes]",null,null,"channel count log",{"$f":"LOG(B6,2)","v":4},"[count]",null,"8bit","Normal","HMAX",355,568,1092]
["Frame Time",{"$f":"G17*G16/1000","v":10.4796},"[ms]",null,null,"HMAX reg",{"$f":"INDIRECT(ADDRESS((G13*2+12)+ISNUMBER(FIND(\"x2\",B5, 2))+ISNUMBER(FIND(\"x2\",B4, 2)), 17-G14))","v":355},"[count]",null,null,"Decimation Xx2","HMAX",356,356,576]
["Max FPS",{"$f":"1000/B15","v":95.423489446162066},"[count]",null,null,"H period",{"$f":"(1/75000000)*1000000*G15","v":4.7333333333333334},"[us]",null,"10bit","Normal","HMAX",375,700,1355]
["Average Transfer Speed",{"$f":"B14/B15*1000","v":853.82190159929758},"[MB/s]",null,null,"VMAX reg",{"$f":"MAX(ROUND((((B9-14.26)/G16)+10), 0), B8+38)","v":2214},"[count]",null,null,"Decimation Xx2","HMAX",375,380,710]
[null,null,null,null,null,"FOT",{"$f":"10*G16","v":47.333333333333336},"[us]",null,"12bit","Normal","HMAX",522,831,1614]
["Exposure times",null,null,null,null,"Readout Time",{"$f":"G16*B8/1000","v":10.299733333333334},"[ms]",null,null,"Decimation Xx2","HMAX",522,522,846]
["Min Exposure Time",{"$f":"ROUND(G15*(1/75000000)*1000000+14.26, 0)","v":19},"[us]"]
["Actual Exposure Time",{"$f":"((ROUND((B9-14.26)/G16,0)*G16)+14.26)/1000","v":1.8993333333333331E-2},"[ms]"]